**CAMERA TRAP DEPLOYMENT DATA SHEET**

Data sheet adapted from the eMammal/Snapshot USA deployment data sheet

**HABITAT\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

FOREST, GRASSLAND, WETLAND, SHORELINE, OTHER (SPECIFY)

**SETTING\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

URBAN, SUBURBAN, RURAL, WILD, OTHER (SPECIFY)

**CAMERA WORKING AT RETRIEVAL? YES\_\_\_\_\_ NO\_\_\_\_\_**

**NOTES:**

**CAMERA DEPLOYMENT STEPS:**

* Check camera date/time are correct and note on sheet.
* Check battery percentage (60% or more).
* Check memory card percentage (should be 0%).
* Clear vegetation within 4ft of the front of the camera.
* Make sure camera is aimed parallel with the ground.
* Secure camera tightly at knee height with locked cable.
* Perform walk test (always) & record detection distance (optional).
* Arm camera and stand in front to take 1st photo.

**CAMERA RETRIEVAL STEPS:**

* Stand in front of camera to take last photo.
* Before powering off, determine camera status. If not working, note reason in comments.
* Power off and retrieve camera and cable.
* Confirm retrieval date and time and note on sheet.

**DETECTION DISTANCE**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_METERS**

**BATTERY PERCENTAGE**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**MEMORY CARD ID**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**CAMERA ID**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**DEPLOYMENT COORDINATES**

USE DECIMAL DEGREES

**LATITUDE\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ LONGITUDE\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**PROJECT/TEAM NAME**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**START DATE\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**START TIME\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**RETRIEVAL DATE\_\_\_\_\_\_\_\_\_\_**

**RETRIEVAL TIME\_\_\_\_\_\_\_\_\_\_**

**DEPLOYMENT NAME**

ex: HBNC.CAM1.04.01.2021

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**